# Argument to the client program is:
# 1. ip-adress to the server
# 2. location to the raw cdr-file
# 3. nanoseconds (0-1000) between writing the buffer to the port
# 4. how many writes to the buffer before the sleep command should accur
# Argument 3 and 4 controlls the flow of the raw cdr-file to the cdrserver

cd $VCDRPATH/bin
# ./client stat181.xxx.com /ext06/data/indata_fraud1/port2file.data.-2089540139 1000 0 &
./client xxx.xxx.xxx.xxx.xxx /export2/home/ndb/vw/data/port2file_data_-2089540139 0 100000 &
