Features
   * Applications using ECC over secp256r1 through the PSA API can use a
     new implementation with a much smaller footprint, but some minor
     usage restrictions. See the documentation of the new configuration
     option MBEDTLS_PSA_P256M_DRIVER_ENABLED for details.
