{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["PIOA","PIOB","PIOC"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PIOA","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"flags":["formulas_cached_only"]}
["PIOA"]
["I/O Line","Peripheral A ","Peripheral B ","Extra Function ","Comments","Label"]
["PA0 ","TIOB0 ","NPCS1 ","WKUP0"]
["PA1 ","TIOA0 ","NPCS2 ","WKUP1","pwm/npcs2","PIN10"]
["PA2 ","TCLK0 ","AD12BTRG ","WKUP2"]
["PA3 ","MCCK ","PCK1"]
["PA4 ","MCCDA ","PWMH0",null,null,"PWMH0"]
["PA5 ","MCDA0","PWMH1",null,null,"PWMH1"]
["PA6 ","MCDA1","PWMH2",null,null,"PWMH2"]
["PA7 ","MCDA2 ","PWML0"]
["PA8 ","MCDA3 ","PWML1"]
["PA9 ","TWD0 ","PWML2 ","WKUP3",null,"SDA1"]
["PA10 ","TWCK0 ","PWML3 ","WKUP4",null,"SCL1"]
["PA11 ","URXD ","PWMFI0",null,null,"RX"]
["PA12 ","UTXD ","PWMFI1",null,null,"TX"]
["PA13 ","MISO",{"$nulls":3},"MISO"]
["PA14 ","MOSI",{"$nulls":3},"MOSI"]
["PA15 ","SPCK ","PWMH2",null,null,"SPCK "]
["PA16 ","NPCS0 ","NCS1 ","WKUP5",null,"NPCS0"]
["PA17 ","SCK0 ","ADTRG ","WKUP6"]
["PA18 ","TXD0 ","PWMFI2 ","WKUP7",null,"TXD0 "]
["PA19 ","RXD0 ","NPCS3 "," WKUP8",null,"RXD0 "]
["PA20 ","TXD1 ","PWMH3 ",null,null,"TXD1 "]
["PA21 ","RXD1 ","PCK0 ","WKUP10",null,"RXD1 "]
["PA22 ","TXD2 ","RTS1 ","AD12B0",null,"TXD2 "]
["PA23 ","RXD2","CTS1",null,null,"RXD2"]
["PA24 ","TWD1","SCK1","WKUP11",null,"SDA0"]
["PA25 ","TWCK1 ","SCK2 ","WKUP12",null,"SCL0"]
["PA26 ","TD ","TCLK2"]
["PA27 ","RD ","PCK0",null,null,"PIN53"]
["PA28","TK","PWMH0",null,null,"PIN38"]
["PA29 ","RK ","PWMH1",null,null,"PIN39"]
["PA30 ","TF ","TIOA2 ","AD12B1",null,"PWM"]
["PA31 ","RF ","TIOB2",null,null,"PIN41"]

{"sheet":"PIOB","index":1,"n_rows":34,"n_cols":6,"rows_kept":34,"flags":["formulas_cached_only"]}
["PIOB"]
["I/O Line","Peripheral A ","Peripheral B ","Extra Function ","Comments","Label"]
["PB0 ","PWMH0 ","A2 ","WKUP13",null,"PIN43"]
["PB1 ","PWMH1 ","A3 ","WKUP14",null,"PIN45"]
["PB2 ","PWMH2 ","A4 ","WKUP15",null,"PIN47"]
["PB3","PWMH3 ","A5","AD12B2",null,"AD8"]
["PB4","TCLK1 ","A6","AD12B3",null,"AD9"]
["PB5 ","TIOA1 ","A7 ","AD0",null,"AD0"]
["PB6","TIOB1 ","D15","AD1",null,"AD1"]
["PB7","RTS0 ","A0/NBS0","AD2",null,"AD2"]
["PB8 ","CTS0","A1","AD3",null,"AD3"]
["PB9 ","D0 ","DTR0",null,null,"DAC-CS"]
["PB10","D1","DSR0",null,null,"DAC-SCK"]
["PB11 ","D2","DCD0",null,null,"PIN49"]
["PB12 ","D3 ","RI0",null,null,"PIN50"]
["PB13 ","D4 ","PWMH0",null,null,"PIN51"]
["PB14","D5","PWMH1",null,null,"DAC-DIN"]
["PB15 ","D6 ","PWMH2"]
["PB16 ","D7 ","PWMH3",null,null,"PWMH3"]
["PB17 ","NANDOE ","PWML0",null,null,"PIN37"]
["PB18 ","NANDWE ","PWML1",null,null,"PIN36"]
["PB19 ","NRD ","PWML2",null,null,"PIN35"]
["PB20 ","NCS0 ","PWML3",null,null,"PIN34"]
["PB21 ","A21/NANDALE ","RTS2",null,null,"PIN33"]
["PB22 ","A22/NANDCLE ","CTS2",null,null,"PIN32"]
["PB23 ","NWR0/NWE ","PCK2",null,null,"PIN31"]
["PB24 ","NANDRDY ","PCK1",null,null,"PIN30"]
["PB25 ","D8 ","PWML0 ",null,null,"PIN29"]
["PB26 ","D9 ","PWML1 ",null,null,"PIN28"]
["PB27 ","D10 ","PWML2 ",null,null,"PIN27"]
["PB28 ","D11 ","PWML3 ",null,null,"PIN26"]
["PB29 ","D12"]
["PB30 ","D13"]
["PB31 ","D14"]

{"sheet":"PIOC","index":2,"n_rows":34,"n_cols":6,"rows_kept":34,"flags":["formulas_cached_only"]}
["PIOC"]
["I/O Line ","Peripheral A ","Peripheral B ","Extra function","Comments","Label"]
["PC0 ","A2",{"$nulls":3},"PIN25"]
["PC1 ","A3",{"$nulls":3},"PIN24"]
["PC2 ","A4",{"$nulls":3},"PIN23"]
["PC3","A5 ","NPCS1",null,null,"PIN22"]
["PC4","A6 ","NPCS2"]
["PC5 ","A7 ","NPCS3 "]
["PC6","A8 ","PWML0",null,null,"PWML0"]
["PC7","A9 ","PWML1",null,null,"PWML1"]
["PC8 ","A10","PWML2",null,null,"PWML2"]
["PC9 ","A11 ","PWML3 ",null,null,"PWML3 "]
["PC10","A12","CTS3 "]
["PC11 ","A13","RTS3"]
["PC12 ","NCS1 ","TXD3 "]
["PC13 ","A2 ","RXD3 "]
["PC14","A3","NPCS2 ",null,null,"RXL"]
["PC15 ","NWR1/NBS1 "," ","AD12B4 ",null,"AD10"]
["PC16 ","NCS2","PWML3","AD12B5 ",null,"AD11"]
["PC17 ","NCS3 ",null,"AD12B6 ",null,"AD12"]
["PC18 ","NWAIT ",null,"AD12B7 ",null,"AD13"]
["PC19 ","SCK3 ","NPCS1 ",null,null,"TXL"]
["PC20 ","A14"]
["PC21 ","A15",{"$nulls":3},"PIN13/LED"]
["PC22 ","A16",{"$nulls":3},"PIN40"]
["PC23","A17",{"$nulls":3},"PIN42"]
["PC24","A18 ","PWMH0",null,null,"PIN44"]
["PC25 ","A19","PWMH1",null,null,"PIN46"]
["PC26","A20 ","PWMH2",null,null,"PIN48"]
["PC27 ","A23 ","PWMH3",null,null,"PIN52"]
["PC28 "," ","MCDA4","AD4 ",null,"AD4 "]
["PC29","PWML0","MCDA5","AD5 ",null,"AD5 "]
["PC30","PWML1 ","MCDA6","AD6 ",null,"AD6 "]
["PC31","PWML2","MCDA7","AD7 ",null,"AD7 "]